What needs to be changed in Simulink file

Battery OCV table data under battery/batteryOCV has to be changed to Battery\_Data\_OCV

Temperature data stays the same, and charging data remains the same, so the route has to be renamed to battery data old along with SOC axis(breakpoints) and temp-axis (breakpoints)

Battery/plant/battery/battery internal resistance/ internal resistance discharging- Battery\_R\_discharge data has to change to SOC\_VS\_IR